<?xml version="1.0" encoding= "UTF-8" ?>
<configuration name="MIMXRT1015-EVK" xsi:schemaLocation="http://mcuxpresso.nxp.com/XSD/mex_configuration_17 http://mcuxpresso.nxp.com/XSD/mex_configuration_17.xsd" uuid="4be4468a-3124-4ac9-9d4f-05d5f8ad6399" version="17" xmlns="http://mcuxpresso.nxp.com/XSD/mex_configuration_17" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
   <common>
      <processor>MIMXRT1015xxxxx</processor>
      <package>MIMXRT1015DAF5A</package>
      <board>MIMXRT1015-EVK</board>
      <board_revision>B</board_revision>
      <mcu_data>ksdk2_0</mcu_data>
      <cores selected="core0">
         <core name="Cortex-M7F" id="core0" description="M7 core"/>
      </cores>
      <description></description>
   </common>
   <preferences>
      <validate_boot_init_only>true</validate_boot_init_only>
      <generate_code_modified_registers_only>false</generate_code_modified_registers_only>
      <update_include_paths>true</update_include_paths>
      <generate_registers_defines>false</generate_registers_defines>
   </preferences>
   <tools>
      <pins name="Pins" version="17.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/pin_mux.c" update_enabled="true"/>
            <file path="board/pin_mux.h" update_enabled="true"/>
         </generated_project_files>
         <pins_profile>
            <processor_version>24.12.10</processor_version>
            <pin_labels>
               <pin_label pin_num="21" pin_signal="GPIO_SD_B1_01" label="GPIO SD_B1_01" identifier="USER_LED"/>
            </pin_labels>
            <external_user_signals>
               <properties/>
            </external_user_signals>
            <power_domains>
               <power_domain name="NVCC_GPIO" value="3.3"/>
            </power_domains>
         </pins_profile>
         <functions_list>
            <function name="BOARD_InitPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="GPIO2" description="Peripheral GPIO2 signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.igpio" description="Pins initialization requires the IGPIO Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="GPIO2" signal="gpio_io, 09" pin_num="1" pin_signal="GPIO_EMC_09">
                     <pin_features>
                        <pin_feature name="direction" value="INPUT"/>
                        <pin_feature name="pull_keeper_select" value="Pull"/>
                        <pin_feature name="pull_up_down_config" value="Pull_Up_47K_Ohm"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="GPIO3" signal="gpio_io, 21" pin_num="21" pin_signal="GPIO_SD_B1_01">
                     <pin_features>
                        <pin_feature name="direction" value="OUTPUT"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
            <function name="BOARD_InitQSPIPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="FLEXSPI" description="Peripheral FLEXSPI signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitQSPIPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitQSPIPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitQSPIPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_SCLK" pin_num="12" pin_signal="GPIO_SD_B1_07"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DATA0" pin_num="11" pin_signal="GPIO_SD_B1_08"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DATA1" pin_num="9" pin_signal="GPIO_SD_B1_10"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DATA2" pin_num="10" pin_signal="GPIO_SD_B1_09"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DATA3" pin_num="13" pin_signal="GPIO_SD_B1_06"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_SS0_B" pin_num="8" pin_signal="GPIO_SD_B1_11"/>
               </pins>
            </function>
            <function name="BOARD_InitDEBUG_UARTPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="LPUART1" description="Peripheral LPUART1 signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitDEBUG_UARTPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitDEBUG_UARTPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitDEBUG_UARTPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="LPUART1" signal="RX" pin_num="68" pin_signal="GPIO_AD_B0_07">
                     <pin_features>
                        <pin_feature name="slew_rate" value="Slow"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="LPUART1" signal="TX" pin_num="72" pin_signal="GPIO_AD_B0_06">
                     <pin_features>
                        <pin_feature name="slew_rate" value="Slow"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
         </functions_list>
      </pins>
      <clocks name="Clocks" version="15.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/clock_config.c" update_enabled="true"/>
            <file path="board/clock_config.h" update_enabled="true"/>
         </generated_project_files>
         <clocks_profile>
            <processor_version>24.12.10</processor_version>
         </clocks_profile>
         <clock_configurations>
            <clock_configuration name="BOARD_BootClockRUN" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.rtc_xtali" description="&apos;RTC_XTALI&apos; (Pins tool id: XTALOSC24M.rtc_xtali, Clocks tool id: XTALOSC24M.RTC_XTALI) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.rtc_xtali" description="&apos;RTC_XTALI&apos; (Pins tool id: XTALOSC24M.rtc_xtali, Clocks tool id: XTALOSC24M.RTC_XTALI) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.rtc_xtalo" description="&apos;RTC_XTALO&apos; (Pins tool id: XTALOSC24M.rtc_xtalo, Clocks tool id: XTALOSC24M.RTC_XTALO) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.rtc_xtalo" description="&apos;RTC_XTALO&apos; (Pins tool id: XTALOSC24M.rtc_xtalo, Clocks tool id: XTALOSC24M.RTC_XTALO) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtali" description="&apos;XTALI&apos; (Pins tool id: XTALOSC24M.xtali, Clocks tool id: XTALOSC24M.XTALI) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtali" description="&apos;XTALI&apos; (Pins tool id: XTALOSC24M.xtali, Clocks tool id: XTALOSC24M.XTALI) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtalo" description="&apos;XTALO&apos; (Pins tool id: XTALOSC24M.xtalo, Clocks tool id: XTALOSC24M.XTALO) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtalo" description="&apos;XTALO&apos; (Pins tool id: XTALOSC24M.xtalo, Clocks tool id: XTALOSC24M.XTALO) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Clocks initialization requires the IOMUXC Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources>
                  <clock_source id="XTALOSC24M.RTC_OSC.outFreq" value="32.768 kHz" locked="false" enabled="true"/>
               </clock_sources>
               <clock_outputs>
                  <clock_output id="AHB_CLK_ROOT.outFreq" value="500 MHz" locked="false" accuracy=""/>
                  <clock_output id="CKIL_SYNC_CLK_ROOT.outFreq" value="32.768 kHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_1M.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_24M.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_500M_REF_CLK.outFreq" value="500 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXIO1_CLK_ROOT.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXSPI_CLK_ROOT.outFreq" value="2160/11 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT1_ipg_clk_highfreq.outFreq" value="62.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT2_ipg_clk_highfreq.outFreq" value="62.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="IPG_CLK_ROOT.outFreq" value="125 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPI2C_CLK_ROOT.outFreq" value="60 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPSPI_CLK_ROOT.outFreq" value="105.6 MHz" locked="false" accuracy=""/>
                  <clock_output id="MQS_MCLK.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="PERCLK_CLK_ROOT.outFreq" value="62.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_CLK_ROOT.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK1.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK2.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK3.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_CLK_ROOT.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK1.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK3.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_CLK_ROOT.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK1.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK3.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="SPDIF0_CLK_ROOT.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="TRACE_CLK_ROOT.outFreq" value="352/3 MHz" locked="false" accuracy=""/>
                  <clock_output id="UART_CLK_ROOT.outFreq" value="80 MHz" locked="false" accuracy=""/>
                  <clock_output id="USBPHY1_CLK.outFreq" value="480 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="CCM.AHB_PODF.scale" value="1" locked="true"/>
                  <setting id="CCM.ARM_PODF.scale" value="1" locked="true"/>
                  <setting id="CCM.CLKO2_SEL.sel" value="CCM.LPI2C_CLK_ROOT" locked="false"/>
                  <setting id="CCM.FLEXSPI_PODF.scale" value="2" locked="true"/>
                  <setting id="CCM.FLEXSPI_SEL.sel" value="CCM_ANALOG.PLL3_PFD0_CLK" locked="false"/>
                  <setting id="CCM.IPG_PODF.scale" value="4" locked="false"/>
                  <setting id="CCM.LPSPI_PODF.scale" value="5" locked="true"/>
                  <setting id="CCM.PERCLK_PODF.scale" value="2" locked="true"/>
                  <setting id="CCM.PRE_PERIPH_CLK_SEL.sel" value="CCM.ARM_PODF" locked="false"/>
                  <setting id="CCM.SEMC_PODF.scale" value="2" locked="false"/>
                  <setting id="CCM.TRACE_PODF.scale" value="3" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2.denom" value="1" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2.num" value="0" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2_BYPASS.sel" value="CCM_ANALOG.PLL2_OUT_CLK" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD0_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD0" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD1_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD2_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD2" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD2_DIV.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2_PFD2_MUL.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2_PFD3_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD3" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD3_DIV.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2_PFD3_MUL.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL3_BYPASS.sel" value="CCM_ANALOG.PLL3" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD0_BYPASS.sel" value="CCM_ANALOG.PLL3_PFD0" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD0_DIV.scale" value="22" locked="true"/>
                  <setting id="CCM_ANALOG.PLL3_PFD0_MUL.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL3_PFD1_BYPASS.sel" value="CCM_ANALOG.PLL3_PFD1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD2_BYPASS.sel" value="CCM_ANALOG.PLL3_PFD2" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD3_BYPASS.sel" value="CCM_ANALOG.PLL3_PFD3" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD3_DIV.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL3_PFD3_MUL.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL4.denom" value="50" locked="false"/>
                  <setting id="CCM_ANALOG.PLL4.div" value="47" locked="false"/>
                  <setting id="CCM_ANALOG.PLL6_BYPASS.sel" value="CCM_ANALOG.PLL6" locked="false"/>
                  <setting id="CCM_ANALOG_PLL_USB1_EN_USB_CLKS_CFG" value="Enabled" locked="false"/>
                  <setting id="CCM_ANALOG_PLL_USB1_EN_USB_CLKS_OUT_CFG" value="Enabled" locked="false"/>
                  <setting id="CCM_ANALOG_PLL_USB1_POWER_CFG" value="Yes" locked="false"/>
               </clock_settings>
               <called_from_default_init>true</called_from_default_init>
            </clock_configuration>
         </clock_configurations>
      </clocks>
      <dcdx name="DCDx" version="3.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <dcdx_profile>
            <processor_version>N/A</processor_version>
         </dcdx_profile>
         <dcdx_configurations/>
      </dcdx>
      <periphs name="Peripherals" version="12.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <peripherals_profile>
            <processor_version>13.0.2</processor_version>
         </peripherals_profile>
         <functional_groups>
            <functional_group name="BOARD_InitPeripherals" uuid="57fc488c-a9f7-4a03-8ab3-5d2a3fd16a50" called_from_default_init="true" id_prefix="" core="core0">
               <description></description>
               <options/>
               <dependencies/>
               <instances>
                  <instance name="DEBUG_UART" uuid="600d7aee-5a2d-4373-9763-ce007b981c15" type="lpuart" type_id="lpuart_bebe3e12b6ec22bbd14199038f2bf459" mode="polling" peripheral="LPUART1" enabled="false" comment="" custom_name_enabled="true" editing_lock="false">
                     <config_set name="lpuartConfig_t" quick_selection="QuickSelection1">
                        <struct name="lpuartConfig">
                           <setting name="clockSource" value="LpuartClock"/>
                           <setting name="lpuartSrcClkFreq" value="ClocksTool_DefaultInit"/>
                           <setting name="baudRate_Bps" value="115200"/>
                           <setting name="parityMode" value="kLPUART_ParityDisabled"/>
                           <setting name="dataBitsCount" value="kLPUART_EightDataBits"/>
                           <setting name="isMsb" value="false"/>
                           <setting name="stopBitCount" value="kLPUART_OneStopBit"/>
                           <setting name="txFifoWatermark" value="0"/>
                           <setting name="rxFifoWatermark" value="1"/>
                           <setting name="enableRxRTS" value="false"/>
                           <setting name="enableTxCTS" value="false"/>
                           <setting name="txCtsSource" value="kLPUART_CtsSourcePin"/>
                           <setting name="txCtsConfig" value="kLPUART_CtsSampleAtStart"/>
                           <setting name="rxIdleType" value="kLPUART_IdleTypeStartBit"/>
                           <setting name="rxIdleConfig" value="kLPUART_IdleCharacter1"/>
                           <setting name="enableTx" value="true"/>
                           <setting name="enableRx" value="true"/>
                        </struct>
                     </config_set>
                  </instance>
                  <instance name="COMBO_SENSOR" uuid="96f9e552-25e5-434a-9454-5cf9e614733d" type="lpi2c" type_id="lpi2c_db68d4f4f06a22e25ab51fe9bd6db4d2" mode="master" peripheral="LPI2C1" enabled="false" comment="" custom_name_enabled="true" editing_lock="false">
                     <config_set name="main" quick_selection="qs_interrupt">
                        <setting name="clockSource" value="Lpi2cClock"/>
                        <setting name="clockSourceFreq" value="ClocksTool_DefaultInit"/>
                        <struct name="interrupt">
                           <setting name="IRQn" value="LPI2C1_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                     </config_set>
                     <config_set name="master" quick_selection="qs_master_transfer">
                        <setting name="mode" value="transfer"/>
                        <struct name="config">
                           <setting name="enableMaster" value="true"/>
                           <setting name="enableDoze" value="true"/>
                           <setting name="debugEnable" value="false"/>
                           <setting name="ignoreAck" value="false"/>
                           <setting name="pinConfig" value="kLPI2C_2PinOpenDrain"/>
                           <setting name="baudRate_Hz" value="100000"/>
                           <setting name="busIdleTimeout_ns" value="0"/>
                           <setting name="pinLowTimeout_ns" value="0"/>
                           <setting name="sdaGlitchFilterWidth_ns" value="0"/>
                           <setting name="sclGlitchFilterWidth_ns" value="0"/>
                           <struct name="hostRequest">
                              <setting name="enable" value="false"/>
                              <setting name="source" value="kLPI2C_HostRequestExternalPin"/>
                              <setting name="polarity" value="kLPI2C_HostRequestPinActiveHigh"/>
                           </struct>
                           <set name="edmaRequestSources">
                              <selected/>
                           </set>
                        </struct>
                        <struct name="transfer">
                           <setting name="blocking" value="false"/>
                           <setting name="enable_custom_handle" value="false"/>
                           <struct name="callback">
                              <setting name="name" value=""/>
                              <setting name="userData" value=""/>
                           </struct>
                           <set name="flags">
                              <selected/>
                           </set>
                           <setting name="slaveAddress" value="0"/>
                           <setting name="direction" value="kLPI2C_Write"/>
                           <setting name="subaddress" value="0"/>
                           <setting name="subaddressSize" value="1"/>
                           <setting name="blocking_buffer" value="false"/>
                           <setting name="enable_custom_buffer" value="false"/>
                           <setting name="dataSize" value="1"/>
                        </struct>
                     </config_set>
                  </instance>
                  <instance name="USER_LED" uuid="5592aac0-ced9-4284-88a8-bbeb5083a92f" type="igpio" type_id="igpio_b1c1fa279aa7069dca167502b8589cb7" mode="GPIO" peripheral="GPIO3" enabled="false" comment="" custom_name_enabled="true" editing_lock="false">
                     <config_set name="fsl_gpio">
                        <setting name="enable_irq_comb_0_15" value="false"/>
                        <struct name="gpio_interrupt_comb_0_15">
                           <setting name="IRQn" value="GPIO3_Combined_0_15_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                        <setting name="enable_irq_comb_16_31" value="false"/>
                        <struct name="gpio_interrupt_comb_16_31">
                           <setting name="IRQn" value="GPIO3_Combined_16_31_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                     </config_set>
                  </instance>
                  <instance name="USER_BUTTON" uuid="e7774953-3606-41b8-8b72-6e09025369e0" type="igpio" type_id="igpio_b1c1fa279aa7069dca167502b8589cb7" mode="GPIO" peripheral="GPIO2" enabled="false" comment="" custom_name_enabled="true" editing_lock="false">
                     <config_set name="fsl_gpio">
                        <setting name="enable_irq_comb_0_15" value="false"/>
                        <struct name="gpio_interrupt_comb_0_15">
                           <setting name="IRQn" value="GPIO2_Combined_0_15_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                        <setting name="enable_irq_comb_16_31" value="false"/>
                        <struct name="gpio_interrupt_comb_16_31">
                           <setting name="IRQn" value="GPIO2_Combined_16_31_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                     </config_set>
                  </instance>
                  <instance name="NVIC" uuid="0329fbca-00e5-4ec4-9f79-3cb65a7b267a" type="nvic" type_id="nvic_57b5eef3774cc60acaede6f5b8bddc67" mode="general" peripheral="NVIC" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="nvic">
                        <array name="interrupt_table"/>
                        <array name="interrupts"/>
                     </config_set>
                  </instance>
               </instances>
            </functional_group>
         </functional_groups>
         <components>
            <component name="system" uuid="59cf1b09-8396-4bf9-bed6-03d5457c292f" type_id="system_54b53072540eeeb8f8e9343e71f28176">
               <config_set_global name="global_system_definitions">
                  <setting name="user_definitions" value=""/>
                  <setting name="user_includes" value=""/>
               </config_set_global>
            </component>
            <component name="msg" uuid="7d589e9f-7522-408c-b7c8-42770920766f" type_id="msg_6e2baaf3b97dbeef01c0043275f9a0e7">
               <config_set_global name="global_messages"/>
            </component>
            <component name="gpio_adapter_common" uuid="e9da5e16-1f55-49be-87ec-af8cfd4a4105" type_id="gpio_adapter_common_57579b9ac814fe26bf95df0a384c36b6">
               <config_set_global name="global_gpio_adapter_common" quick_selection="default"/>
            </component>
            <component name="generic_uart" uuid="9dc7a034-9408-4852-9990-a713693635ee" type_id="generic_uart_8cae00565451cf2346eb1b8c624e73a6">
               <config_set_global name="global_uart"/>
            </component>
            <component name="generic_can" uuid="28ec81a8-d7ea-4363-9330-20b877c481f6" type_id="generic_can_1bfdd78b1af214566c1f23cf6a582d80">
               <config_set_global name="global_can"/>
            </component>
            <component name="uart_cmsis_common" uuid="774dd0a0-63ed-4846-b9d7-dfd082d810e3" type_id="uart_cmsis_common_9cb8e302497aa696fdbb5a4fd622c2a8">
               <config_set_global name="global_USART_CMSIS_common" quick_selection="default"/>
            </component>
            <component name="generic_enet" uuid="77cd333e-4adc-4c6e-8b18-bbe349d78182" type_id="generic_enet_74db5c914f0ddbe47d86af40cb77a619">
               <config_set_global name="global_enet"/>
            </component>
         </components>
      </periphs>
      <tee name="TEE" version="4.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <tee_profile>
            <processor_version>N/A</processor_version>
         </tee_profile>
      </tee>
   </tools>
</configuration>
