/*###ICF### Section handled by ICF editor, don't touch! ****/
/*-Editor annotation file-*/
/* IcfEditorFile="$TOOLKIT_DIR$\config\ide\IcfEditor\cortex_v1_0.xml" */
/*-Specials-*/
define symbol __ICFEDIT_intvec_start__ = 0x08000000;
/*-Memory Regions-*/
define symbol NONCACHEABLEBUFFER_size   = 0x4000;
define symbol __ICFEDIT_region_ROM_start__ = 0x08000000;
define symbol __ICFEDIT_region_ROM_end__   = 0x0800FFFF;
define symbol __ICFEDIT_region_RAM_start__ = 0x24000000;
define symbol __ICFEDIT_region_RAM_end__   = 0x2404FFFF - NONCACHEABLEBUFFER_size;
define symbol NONCACHEABLEBUFFER_start     = __ICFEDIT_region_RAM_end__ + 1;
define symbol NONCACHEABLEBUFFER_end       = __ICFEDIT_region_RAM_end__ + NONCACHEABLEBUFFER_size;


/*-Sizes-*/
define symbol __ICFEDIT_size_cstack__ = 0x800;
define symbol __ICFEDIT_size_heap__   = 0x200;
/**** End of ICF editor section. ###ICF###*/

define symbol __region_ITCM_start__ = 0x00000000;
define symbol __region_ITCM_end__   = 0x0000FFFF;
define symbol __region_DTCM_start__ = 0x20000000;
define symbol __region_DTCM_end__   = 0x2000FFFF;
define symbol __region_SRAMAHB_start__ = 0x30000000;
define symbol __region_SRAMAHB_end__   = 0x30007FFF;
define symbol __region_BKPSRAM_start__ = 0x38800000;
define symbol __region_BKPSRAM_end__   = 0x38800FFF;

export symbol NONCACHEABLEBUFFER_start;
export symbol NONCACHEABLEBUFFER_size;

export symbol __ICFEDIT_region_ROM_start__;
export symbol __ICFEDIT_region_ROM_end__;
define memory mem with size = 4G;
define region ROM_region      = mem:[from __ICFEDIT_region_ROM_start__ to __ICFEDIT_region_ROM_end__];
define region RAM_region      = mem:[from __ICFEDIT_region_RAM_start__ to __ICFEDIT_region_RAM_end__];
define region NONCACHEABLE_region   = mem:[from NONCACHEABLEBUFFER_start to NONCACHEABLEBUFFER_end];
define region ITCM_region     = mem:[from __region_ITCM_start__ to __region_ITCM_end__];
define region DTCM_region     = mem:[from __region_DTCM_start__ to __region_DTCM_end__];
define region SRAMAHB_region  = mem:[from __region_SRAMAHB_start__ to __region_SRAMAHB_end__];
define region BKPSRAM_region  = mem:[from __region_BKPSRAM_start__ to __region_BKPSRAM_end__];

define block CSTACK    with alignment = 8, size = __ICFEDIT_size_cstack__   { };
define block HEAP      with alignment = 8, size = __ICFEDIT_size_heap__     { };

initialize by copy { readwrite };
do not initialize  { section .noinit };

place at address mem:__ICFEDIT_intvec_start__ { readonly section .intvec };

place in ROM_region   { readonly };
place in RAM_region   { readwrite };
place in NONCACHEABLE_region { section noncacheable_buffer };
place in DTCM_region  { block CSTACK, block HEAP };
